PROJECT OPENSKY BOEING 737-800 PROCEDURES
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 340 KIAS
MMO - Maximum Operating Speed Mach | .82 Mach
Turbulent Air Penetration Speed | 280 KIAS/.73 Mach
VLO - Maximum Gear Operating Speed | 235 KIAS
VLE - Maximum Landing Gear Extension Speed | 270 KIAS/.82 Mach

Maximum Flap Placard Speeds

Flaps degrees | KIAS
1 | 230
2 | 230
5 | 225
10 | 210
15 | 195
25 | 190
30 | 185
40 | 158

V1 - Takeoff Decision Speed dry runway; flaps 5
Standard temperature, sea level pressure altitude

143,000 lbs | 150 KIAS
132,000 lbs | 143 KIAS

Standard temperature, 5,000' pressure altitude

143,000 lbs | 152 KIAS
132,000 lbs | 145 KIAS

VR - Rotation Speed dry runway, flaps 5
Standard temperature, sea level pressure altitude

143,000 lbs | 154 KIAS
132,000 lbs | 147 KIAS

Standard temperature, 5,000' pressure altitude

143,000 lbs | 157 KIAS
132,000 lbs | 149 KIAS

V2 - Takeoff Safety Speed dry runway, flaps 5
Standard temperature, sea level pressure altitude

143,000 lbs | 162 KIAS
132,000 lbs | 155 KIAS

Standard temperature, 5,000' pressure altitude

143,000 lbs | 161 KIAS
132,000 lbs | 155 KIAS

VREF - Landing Approach Speed flaps 30, gear down

136,400 lbs | 147 KIAS
132,000 lbs | 144 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.